EMpower and Firmware v2.48.0 Release Notes
Nov 04 2025
=======================================
	Operating systems supported
=======================================
Windows
        * Permissions required: Must be logged in as Administrator
        * Versions tested:
                - Windows 10, 64-bit
                - Windows 11, 64-bit
        * NOTE: Windows 10S and Windows 11S are not supported
Linux
        * Permissions required: Standard user
        * Versions tested:
                - Ubuntu 20.04.4
Mac
        * Permissions required: Standard User
        * Versions tested:
                - macOS 10.15.4, Catalina
                - macOS 12.0 (Monterey - Apple Silicon)
                - macOS  14.4 (Sonoma)
=======================================
What's new in the Latest Version
=======================================

== System Enhancements ==

*MTU-5C systems (model RMT08 and higher, with bootloaders shipped after October 2025, version 0x00001A) now allow automatic restart after a shutdown that protects the receiver from overheating. For more specific identification, please consult the Power Recovery Manual.
* MTU-5C systems (model RMT08 and higher) now allow powering off the Ethernet port to reduce heat and power.

== EMpower New Features ==
* Added "Delete" key support to the Time-Based Editing Plot in the EMpower MT editor to delete selected time masks.

== EMpower Bug Fixes ==
* Fixed an issue causing all map recordings to become selectable when toggling between world and local views. 
* Fixed an issue in EMpower Manage causing recordings that are disabled in the map to be re-enabled for selection when the map is switched between world and local views.
* Fixed an issue where setting the grid position to 0,0 and switching the viewport to the local (UTM) map caused the map to become unresponsive and, in some cases, crash.
* Fixed an issue where right-clicking the calibration check icon after selecting a recording on the timeline caused a crash.
* Standardized x-axis labels and ticks in the receiver calibration viewer across all zoom levels.
=====================================
Known Issues for the Latest version:
=====================================
* Low frequency PNT(<100s) may have some issues with full rate recordings
* Mixed use of real and generic receiver calibrations could potentially distort phase curves at high frequencies
* If a config file for remote control is created and saved, the network checkmark in EMpower config creator does not turn off automatically the next time, unless the user manually unchecks the remote control server.

***IMPORTANT***
** Please do not open any project in an EMpower version older than 1.54.x.x if the project has already been opened in this version