EMpower and Firmware v2.56.0 Release Notes
May 28 2026
=======================================
	Operating systems supported
=======================================
Windows
        * Permissions required: Must be logged in as Administrator
        * Versions tested:
                - Windows 10, 64-bit
                - Windows 11, 64-bit
        * NOTE: Windows 10S and Windows 11S are not supported
Linux
        * Permissions required: Standard user
        * Versions tested:
                - Ubuntu 20.04.4
                - Ubuntu 24.04.4
Mac
        * Permissions required: Standard User
        * Versions tested:
                - macOS 10.15.4, Catalina
                - macOS 12.0 (Monterey - Apple Silicon)
                - macOS  14.4 (Sonoma)
=======================================
What's new in the Latest Version
=======================================

== System Enhancements ==

●	Firmware support for V9 receiver systems
●	Supporting TDEM in V9 receivers and TXD-1 transmitter drivers
●	New receivers such as V9 and future MTU-5CDS receivers (model RTM08-B to be released soon) have been improved to support a higher internal temperature cutoff at 75°C

== EMpower New Features ==
●	Added support for the new multifunction, multi-physics V9 receiver. EMpower now configures the V9 receiver, imports and processes V9 data, and visualizes results for CSAMT, MT, PNT, and TDEM techniques.
●	Added support for TDEM recordings, including support in Field QC, Recording Library, Processed TDEM Data Viewer tab, TDEM Stack Editor, TDEM metadata export, and TDEM processed site export.
●	Added CPU temperature monitoring for V9 receivers and MTU-5C receivers of models RMT08-A and above
●	Improved PNT setup dialog to enable selection of up to 7 channels in any combination.
== EMpower Bug Fixes ==
●	Fixed GLONASS constellation being automatically enabled when loading a config file